🏠
Max Site
ISP: Brightspeed Fiber → Coax
Edge Router / Firewall
🔥 Magikarp "The Router from Hell" 10GbE ROUTER
Platform:Gentoo Linux / AMD Ryzen 5700G 8C/16T
RAM:32GB DDR4 3600MHz
NIC:Intel X710 2x10G SFP+
WAN:enp34s0f0np0 - DHCP/25
LAN:enp34s0f1np1 - 192.168.1.1/24
VLAN 20:192.168.8.1/24 (Garnpmet/IoT)
VLAN 77:172.20.8.1/24 (HPBX)
WireGuard:10.10.10.1/32 | 172.16.20.3/24
OSPF ID:10.10.10.1 | Area 0.0.0.0
OSPF WireGuard 10GbE
Network Infrastructure
🔌 Netgear Cable Modem MODEM
IP:192.168.100.1/32
🔀 Switchfish - TP-Link SG2210P L2+ SWITCH
Main VLAN:192.168.1.20/24
VLAN 20:192.168.8.20/24
VLAN 777:172.20.8.20/24
Access Points / Sub-Routers
📶 WiFiSlab - Mikrotik cAP ax AP/ROUTER
Main:192.168.1.15/24
VLAN 20:192.168.8.15/24
Subnet:192.168.20.1/24 | 192.168.11.1/24
📶 Macrohard - Mikrotik RB2011UiAS-RM ROUTER
Main:192.168.1.30/24
VLAN 20 WAN:192.168.8.30/24
VLAN 777 WAN:172.20.8.30/24
Subnets:192.168.88.1/24 | 192.168.10.1/24 | 172.20.10.1/24
Server Cluster
🐧 Gyarados
192.168.1.199/24
Main Server | Bridge: 192.168.1.221/24
🐟 Zfish
192.168.1.158/24
Head Unit / Controller
🌐 Pleco
192.168.1.125/24
Web Server | WAN Facing
🐱 Catfish
192.168.1.110/24
Hosting Server | WAN Facing
💻 Loach
192.168.1.109/24
Debian Workstation
🐧 Linux Testing VM
DHCP/24
Test Environment
☁️
Internet
← Brightspeed Network
+ WireGuard P2P
Socket Telecom Fiber →
+ WireGuard P2P
🔐 WireGuard OSPF Mesh
Max (Spoke)
10.10.10.1
172.16.20.3
Jeff (Hub)
10.10.20.1
172.16.20.1
Linda (Spoke)
10.10.40.1
172.16.20.2
🏡
Linda Site
ISP: Socket Telecom Fiber
Edge / ONT
📡 Adtran 611 ONT ONT
Router
📶 Lindarotik - Mikrotik hAP ax3 ROUTER
WAN:DHCP
LAN:192.168.25.1/24
WireGuard:10.10.40.1/32
Transit:172.16.20.2/24
OSPF ID:10.10.40.1 | Area 0.0.0.0
OSPF WireGuard
Mesh APs
📶 TP-Link Deco X50 Mesh MESH AP
IPs:192.168.25.246/24, .247/24
🌐
Gateway Site (Jeff/Dad)
ISP: Socket Telecom Fiber | WG HUB
Edge / ONT
📡 Adtran 411 ONT ONT
Hub Router
🌐 Jeffrotik - Mikrotik hAP ax2 HUB ROUTER
WAN:DHCP
LAN:192.168.5.1/24
Dad VLAN:192.168.30.1/24 (VLAN 30)
WireGuard:10.10.20.1/32
Transit:172.16.20.1/24
Road Warrior:10.10.90.1/24
OSPF ID:10.10.20.1 | Area 0.0.0.0
OSPF HUB WireGuard
Access Points
📶 WiScience Fiction - Mikrotik cAP ax AP
IP:192.168.5.23/24

### 📊 Network Summary

#### 🔗 ISP Connections

Max Site: Brightspeed Fiber → Coax
Linda Site: Socket Telecom Fiber
Gateway Site: Socket Telecom Fiber

#### 🔐 WireGuard + OSPF

Topology: Hub-and-Spoke (Jeff = Hub)
Transit Network: 172.16.20.0/24
OSPF Area: 0.0.0.0 (Backbone)
Type: Point-to-Multipoint + Static Neighbors

#### 🔥 Router from Hell Specs

CPU: AMD Ryzen 7 5700G (8C/16T @ 4.6GHz)
RAM: 32GB DDR4 3600MHz
NIC: Intel X710 2x10G SFP+
OS: Gentoo Linux (nftables + Bird2 + WireGuard)
Offload: nftables flowtable + TSO/GSO/GRO

#### 📝 Recent Changes

✅ Completed:
• NanoPi R5C → Magikarp "Router from Hell" migration
• Magikarp removed from server cluster
• 10GbE backbone ready for Socket Fiber
📋 Pending:
• NanoPi R5C repurposed for new site